1.Before upgrade the software firmware, you need a USB drive, and then copy the software firmware zip file(LB.tar.xz) to the USB drive.
2.Insert the USB drive containing the copied software firmware into the USB port on the case.
3.Complete the upgrade by following the steps in the video.